# General Usage Instructions

Mortise and Tenon creates a mortise and tenon joint between two boards. This add-in allows you to specify the dimensions and location of the joint. It is particularly useful in woodworking.

Steps:

1. Press the Mortise and Tenon button in the Modify panel.
2. Select a board to cut the mortise.
3. Select a face for the tenon.
4. Specify the joint depth, length, thickness, offsets, and number of tenons.
5. To create constrained geometry check the Constrained checkbox in Settings. The constrained geometry calculates longer, but it better follows the changes in the board and face dimensions.
6. Press the OK button.

Help online: https://maciejrogowski.com/mortise-and-tenon-help/

# Version

1.2.0

# Support Information

For support please email: info@maciejrogowski.com

# Author/Company Information

Company Name: Maciej Rogowski
Company URL: https://maciejrogowski.com/

# Privacy Policy

Privacy Policy: https://maciejrogowski.com/add-ins-privacy-policy/